#######################################################################
# parametres pour INCA
#######################################################################
#LMDZ_10m_winds=y --> use 10m wind from LMDZ, =n --> use 10m wind from output file
LMDZ_10m_winds=_AUTO_
10m_winds_method=_AUTO_
#freq_write_chem --> write frequency for inca_inst and inca_avgr (86400 = 1/day)
freq_write_chem=_AUTO_
#choose if there is a feedback with the areosol effect
feedb=_AUTO_
#indicate if we are running with xios and/or ioipsl
XIOS_INCA_OK=_AUTO_
IOIPSL_INCA_OK=_AUTO_
#weibull 10m wind parameter
kref=4.0
#threshold 10m wind parameter
tref=0.85
#sedimentation 
multilayer_sediment=_AUTO_
#coupled model with orchidee
CoupOrchInca=_AUTO_
#use or not the deposition from orchidee
DepOrch=n
# uncomment two next line if we want to coupled with orchidee without transfer any flux
#nbFlux_FromOrch=0
#emi_FromOrch=
#output diagnostic for chemistry flux
calcul_flux=_AUTO_
#
flag_plume=0
#choose which type of aircraft you will use (0 - 1 - 2 - 3) (no aircraft / old inca aircraft / new subsonic inca aircraft / subsonic + hypersonic inca aircraft)
flag_plane=1
#choose if you want or not a time interpolation to use emission flux 
emi_interp_time=1
