orchidee.def

_ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ 
|  0   orchidee.def
- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - 
0#
0#**************************************************************************
0#                    Parameter file list for ORCHIDEE
0# See all optional parameters in modipsl/modeles/ORCHIDEE/orchidee.default
0#**************************************************************************
0
0# Input and output
0#**************************************************************************
0# Restart the time from the GCM. 
0# default = n
0SECHIBA_reset_time = y
0
0# Name of restart to read for initial conditions
0# default = NONE
0SECHIBA_restart_in= sechiba_rest_in.nc
0
0# Name of restart to read for initial conditions of STOMATE
0# default = NONE
0STOMATE_RESTART_FILEIN= stomate_rest_in.nc
0
0# Use XIOS for writing diagnostics file
0# default = y
0XIOS_ORCHIDEE_OK = y
0
0# Writefrequency in seconds in sechiba_history.nc
0# default = 0
0WRITE_STEP = 0
0
0# Print level for text output in out_orchidee_*
0# PRINTLEV = 1 : some output in initialization phase
0# PRINTLEV = 2 : more output in initialization phase and printing of new date
0# PRINTLEV = 3, 4,.. : more output also at each timestep
0PRINTLEV=1
0
0# Hydrology parameters
0#**************************************************************************
0# Activate the multi-layer diffusion scheme adapted from CWRR
0# default = y
0HYDROL_CWRR = y
0
0# Activate river routing
0# default = y
0RIVER_ROUTING = y
0
0# Activate creation of river_desc.nc file
0# RIVER_DESC will be activated only the first execution in the simulation. 
0RIVER_DESC= n
0
0# SOILTYPE_CLASSIF :  Type of classification used for the map of soil types (default zobler)
0SOILTYPE_CLASSIF = zobler 
0SOILALB_FILE     = soils_param.nc
0SOILCLASS_FILE   = soils_param.nc
0
0# DO_RSOIL : Reduce soil evaporation with a soil resistance (default n)
0DO_RSOIL = n
0
0# To make AVAN and NVAN constant with depth (default CWRR_AKS_A0=0, CWRR_AKS_POWER=0, CWRR_NKS_A0=0, CWRR_NKS_POWER=0 )
0CWRR_AKS_A0 = 0.
0CWRR_AKS_POWER = 0.
0CWRR_NKS_A0 = 0.
0CWRR_NKS_POWER = 0.
0
0#**************************************************************************
0# Activate Stomate component
0STOMATE_OK_STOMATE= y
0
0# Activate calculations of CO2 according to Farqhuar and Ball
0# default = y
0STOMATE_OK_CO2 = y
0
0# CDRAG_from_GCM: Use cdrag coefficient from gcm (default=y if coupled to LMDZ)
0CDRAG_from_GCM = y
0
0# Interception reservoir coefficient.
0# default = 0.1
0SECHIBA_QSINT = 0.02
0
0# Use 15 PFTs. Note that PFTmap.nc must contains 15PFTs.
0# PFT=10, 14 and 15 share the same parametrization except for VCMAX and LAI_MAX specified below.  
0NVM=15
0PFT_TO_MTC=1,2,3,4,5,6,7,8,9,10,11,12,13,10,10
0PFT_NAME__10='temperate C3           grass      '
0PFT_NAME__14='tropical  C3           grass      '
0PFT_NAME__15='boreal    C3           grass      '
0
0# STRESS_GS, STRESS_GM, STRESS_VCMAX : Stress on GS, GM and VCMAX
0# Default STRESS_GS=1, STRESS_GM=1, STRESS_VCMAX=1 for all PFTs
0STRESS_GS=1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.
0STRESS_GM=1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.
0STRESS_VCMAX=1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.
0
0# Optimized parameters for albedo (default values)
0ALB_LEAF_NIR = 0.,0.23,0.18,0.18,0.20,0.24,0.15,0.26,0.20,0.24,0.27,0.28,0.26,0.24,0.24
0ALB_LEAF_VIS = 0.,0.04,0.04,0.04,0.04,0.03,0.03,0.03,0.03,0.06,0.06,0.06,0.06,0.06,0.06
0SNOWA_AGED_NIR = 0.50,0,0,0.10,0.37,0.08,0.16,0.17,0.27,0.44,0.44,0.44,0.44,0.44,0.44
0SNOWA_DEC_NIR = 0.13,0,0,0.10,0.10,0.16,0.04,0.07,0.08,0.12,0.12,0.12,0.12,0.12,0.12
0SNOWA_AGED_VIS = 0.74,0,0,0.08,0.24,0.07,0.18,0.18,0.33,0.57,0.57,0.57,0.57,0.57,0.57
0SNOWA_DEC_VIS = 0.21,0,0,0.14,0.08,0.17,0.05,0.06,0.09,0.15,0.15,0.15,0.15,0.15,0.15
0
0# Optimized parameters for photosynthetic capacity 
0# Default values except for PFT=15
0VCMAX25__02 = 45.0
0VCMAX25__03 = 45.0
0VCMAX25__04 = 35.0
0VCMAX25__05 = 40.0
0VCMAX25__06 = 50.0
0VCMAX25__07 = 45.0
0VCMAX25__08 = 35.0
0VCMAX25__09 = 35.0
0VCMAX25__10 = 50.0
0VCMAX25__11 = 50.0
0VCMAX25__12 = 60.0
0VCMAX25__13 = 60.0
0VCMAX25__14 = 50.0
0VCMAX25__15 = 40.0
0
0# Optimized parameters for LAI
0# Default values except for PFT=15
0LAI_MAX__02 = 7.0
0LAI_MAX__03 = 5.0
0LAI_MAX__04 = 5.0
0LAI_MAX__05 = 4.0
0LAI_MAX__06 = 5.0
0LAI_MAX__07 = 3.5
0LAI_MAX__08 = 4.0
0LAI_MAX__09 = 3.0
0LAI_MAX__10 = 2.5
0LAI_MAX__11 = 2.0
0LAI_MAX__12 = 5.0
0LAI_MAX__13 = 5.0
0LAI_MAX__14 = 2.5
0LAI_MAX__15 = 2.0
0
0# Activate downregulation for CO2
0DOWNREGULATION_CO2=y
0DOWNREGULATION_CO2_BASELEVEL=380.
0
0# Activate harvest of wood
0DO_WOOD_HARVEST= y
0
0# Growth respiration (default values except for PFT=14 and PFT=15)
0FRAC_GROWTHRESP__02 = 0.35
0FRAC_GROWTHRESP__03 = 0.35
0FRAC_GROWTHRESP__04 = 0.28
0FRAC_GROWTHRESP__05 = 0.28
0FRAC_GROWTHRESP__06 = 0.28
0FRAC_GROWTHRESP__07 = 0.35
0FRAC_GROWTHRESP__08 = 0.35
0FRAC_GROWTHRESP__09 = 0.35
0FRAC_GROWTHRESP__10 = 0.28
0FRAC_GROWTHRESP__11 = 0.28
0FRAC_GROWTHRESP__12 = 0.28
0FRAC_GROWTHRESP__13 = 0.28
0FRAC_GROWTHRESP__14 = 0.35
0FRAC_GROWTHRESP__15 = 0.35
0
0# Maintenance respiration slope C (default values except for PFT=14 and PFT=15)
0MAINT_RESP_SLOPE_C__02 = 0.12
0MAINT_RESP_SLOPE_C__03 = 0.12
0MAINT_RESP_SLOPE_C__04 = 0.16
0MAINT_RESP_SLOPE_C__05 = 0.16
0MAINT_RESP_SLOPE_C__06 = 0.16
0MAINT_RESP_SLOPE_C__07 = 0.25
0MAINT_RESP_SLOPE_C__08 = 0.25
0MAINT_RESP_SLOPE_C__09 = 0.25
0MAINT_RESP_SLOPE_C__10 = 0.16
0MAINT_RESP_SLOPE_C__11 = 0.12
0MAINT_RESP_SLOPE_C__12 = 0.16
0MAINT_RESP_SLOPE_C__13 = 0.12
0MAINT_RESP_SLOPE_C__14 = 0.12
0MAINT_RESP_SLOPE_C__15 = 0.25
0
0# Soil turnover (default CARBON_TAU=7, CARBON_TAU_IPASSOVE=300)
0CARBON_TAU_ISLOW = 7
0CARBON_TAU_IPASSIVE = 300
0
0# Take carbon from atmosphere if carbohydrate reserve too small, PFT dependent
0# Set to y for all pft except C4 grass (pft=11) and tropical C3 grass (pft=14)
0ALWAYS_INIT =  y, y, y, y, y, y, y, y, y, y, n, y, y, n, y
0
0# Do not use default fire module
0# Default FIRE_DISABLE=y
0FIRE_DISABLE = y
0
0# Parameters related to vegetation map
0#**************************************************************************
0# Update vegetation frequency
0# The maximum vegetation fractions will be update at this period
0# default = 1Y
0VEGET_UPDATE= n
0
0# Read lai map (default n)
0LAI_MAP=  n
0
0# Parameters related to surface and thermal physical properties
0#************************************************************************
0# Read bare soil albedo from file with background MODIS data
0# Default ALB_BG_MODIS=y
0ALB_BG_MODIS = y
0ALB_BG_FILE  = alb_bg.nc
0
0# ROUGH_DYN : Account for a dynamic roughness height (activation of Su et al. parametrization) (default y)
0ROUGH_DYN=y
0
0# OK_FREEZE :  Activate the complet soil freezing scheme (default y)
0OK_FREEZE=y
0
0# DEPTH_MAX_T (m) :  Maximum depth of the soil thermodynamics (default 90)
0DEPTH_MAX_T=90
0
0# OK_EXPLICITSNOW :  Activate explict snow scheme (default y)
0OK_EXPLICITSNOW=y
0 
0# READ_REFTEMP :  Initialize soil temperature using climatological temperature (default y if OK_FREEZE=y)
0READ_REFTEMP=y
0
0# Parameters related to chemistry bvoc 
0#************************************************************************
0# CHEMISTRY_OK_BVOC :  Activate chemistry
0CHEMISTRY_BVOC =  n
0
0# CO2 FOR BVOC - WILKINSON :  CO2 inhibition effect for isoprene based on Wilkinson approach?
0CO2_FOR_BVOC_WILKINSON=n
0
0# CO2 FOR BVOC - POSSELL :  CO2 inhibition effect for isoprene based on Possell approach?
0CO2_FOR_BVOC_POSSELL=n
0

