#
#
# Parameter file for IPSLCM4_v2 configuration
# See comments : http://forge.ipsl.jussieu.fr/orchidee/
#
STOMATE_OK_CO2=TRUE
# STOMATE_OK_STOMATE is not set
# STOMATE_OK_DGVM is not set
# STOMATE_WATCHOUT is not set
SECHIBA_restart_in=_start_sech_
SECHIBA_rest_out=sechiba_rest.nc
SECHIBA_reset_time=y
# SECHIBA_reset_time is not set
OUTPUT_FILE=sechiba_out.nc
WRITE_STEP=2592000
SECHIBA_HISTLEVEL=5
STOMATE_OUTPUT_FILE=stomate_history.nc
STOMATE_HIST_DT=10.
STOMATE_HISTLEVEL=0
SECHIBA_DAY=0.0
SECHIBA_ZCANOP=0.5
DT_SLOW=86400.
# IMPOSE_VEG is not set
VEGETATION_FILE=carteveg5km.nc
# VEGETATION_FILE=pft_new.nc
DIFFUCO_LEAFCI=233.
CONDVEG_SNOWA=default
# IMPOSE_AZE is not set
SOILALB_FILE=soils_param.nc
SOILTYPE_FILE=soils_param.nc 
ENERBIL_TSURF=280.
HYDROL_SNOW=0.0
HYDROL_SNOWAGE=0.0
HYDROL_SNOWICE=0.0
HYDROL_SNOWICEAGE=0.0
HYDROL_HDRY=1.0
HYDROL_HUMR=1.0
HYDROL_BQSB=default
HYDROL_GQSB=0.0
HYDROL_DSG=0.0
HYDROL_DSP=default
HYDROL_QSV=0.0
HYDROL_OK_HDIFF=n
HYDROL_TAU_HDIFF=1800.
THERMOSOIL_TPRO=280.
RIVER_ROUTING=y
ROUTING_FILE=routing.nc
LAI_MAP=y
LAI_FILE=lai2D.nc
SECHIBA_QSINT=0.02
ALB_BARE_MODEL = FALSE
PERCENT_THROUGHFALL_PFT = 30., 30., 30., 30., 30., 30., 30., 30., 30., 30., 30., 30., 30.
RVEG_PFT = .5, .5, .5, .5, .5, .5, .5, .5, .5, .5, .5, .5, .5
CDRAG_FROM_GCM = .TRUE.
#LAND_USE=y
#VEGET_YEAR=0
#VEGET_UPDATE=1Y
