#######################################################################
# parametres pour INCA
#######################################################################
#LMDZ_10m_winds=y --> use 10m wind from LMDZ, =n --> use 10m wind from output file
LMDZ_10m_winds=_AUTO_
#choose if there is a feedback with the areosol effect
feedb=_AUTO_
#threshold 10m wind parameter / def 0.78
tref=_AUTO_: DEFAULT =0.78
#seasalt_correctif / def = 1 
ss_corr=_AUTO_: DEFAULT =1 
#coupled model with orchidee
CoupOrchInca=_AUTO_: DEFAULT=n
nbveget=15
#use or not the deposition from orchidee
DepOrch=n
# uncomment two next line if we want to coupled BVOC flux with orchidee without transfer any flux
nbFlux_BVOC_FromOrch=0
#emi_BVOC_FromOrch=
# uncomment two next line if we want to coupled Nsoil with orchidee without transfer any flux
nbFlux_N_FromOrch=0
#emi_N_FromOrch=n2o
#output diagnostic for chemistry flux
calcul_flux=_AUTO_
#
flag_plume=0
#choose which type of aircraft you will use (0 - 1 - 2 - 3) (no aircraft / old inca aircraft / new subsonic inca aircraft / subsonic + hypersonic inca aircraft)
flag_plane=_AUTO_
#choose which time interpolation you want to interpolate sflx file. ( 0 - 1 - 2) (no interpolation / point to point interpolation / Sheng & Zwiers interpolation) 
emi_interp_time=_AUTO_: DEFAULT=1
#activate reading of sflx_NAT.nc file by year and with separate sources (oce, land, misc) for emissions
multi_sources_nat=_AUTO_: DEFAULT=n
#activate the flag cmip_xml if you are running a CMIP experiment
cmip_xml=_AUTO_: DEFAULT =n
xios_read=_AUTO_: DEFAULT =n
#coupled model with pisces
CoupOceAtm=_AUTO_: DEFAULT=n
transm_dms_oa=_AUTO_: DEFAULT=n
transm_n2o_oa=_AUTO_: DEFAULT=n

