&params_run
duration='1d'
nb_proc_atm=1
/
