#
# Namelist for ORCHIDEE
#
#
#************************************************************************************
# Parametrization :
#------------------------------------------------------------------------------------
STOMATE_OK_CO2=y
STOMATE_OK_STOMATE=n
STOMATE_OK_DGVM=n
LPJ_GAP_CONST_MORT=y
#
# Model chatting level
#------------------------------------------------------------------------------------
BAVARD=1
ALMA_OUTPUT=n
# To reset the time coming from SECHIBA restart file
#------------------------------------------------------------------------------------
SECHIBA_reset_time=y
#
#************************************************************************************
#          Files : incoming / forcing / restart /output
#************************************************************************************
# Ancillary files :
#------------------------------------------------------------------------------------
VEGETATION_FILE=carteveg5km.nc
SOILALB_FILE=soils_param.nc
SOILTYPE_FILE=soils_param.nc
ROUTING_FILE=routing.nc
REFTEMP_FILE=reftemp.nc
LAI_FILE=lai2D.nc
#
# Forcing file name
FORCING_FILE=Cabauw.nc
#
# Input and output restart file for the driver
#------------------------------------------------------------------------------------
RESTART_FILEIN=default
RESTART_FILEOUT=driver_rest_out.nc
#
# Input and output restart file for SECHIBA :
#------------------------------------------------------------------------------------
SECHIBA_restart_in=NONE
SECHIBA_rest_out=sechiba_rest_out.nc
#
# Input and output restart file for STOMATE :
#------------------------------------------------------------------------------------
STOMATE_RESTART_FILEIN=NONE
STOMATE_RESTART_FILEOUT=stomate_rest_out.nc
#
# Forcing files for TESTSTOMATE and FORCESOIL
#------------------------------------------------------------------------------------
STOMATE_FORCING_NAME=stomate_forcing.nc
STOMATE_CFORCING_NAME=stomate_Cforcing.nc
#
# Output file name (SECHIBA puis STOMATE) :
#------------------------------------------------------------------------------------
OUTPUT_FILE=sechiba_history.nc
STOMATE_OUTPUT_FILE=stomate_history.nc
#
# Write levels for outputs files (number of variables) :
#------------------------------------------------------------------------------------
SECHIBA_HISTLEVEL=5
STOMATE_HISTLEVEL=10
#
# Write frequency for output files (SECHIBA in seconds et
# STOMATE in days) :
#------------------------------------------------------------------------------------
WRITE_STEP=1800.0
STOMATE_HIST_DT=10.
#
#************************************************************************************
#                             Area location
#************************************************************************************
LIMIT_WEST=-180.
LIMIT_EAST=180.
LIMIT_NORTH=90.
LIMIT_SOUTH=-90.
##************************************************************************************
#                       Simulation parameters
#************************************************************************************
# Weather generator or not :
#------------------------------------------------------------------------------------
ALLOW_WEATHERGEN=y
IPPREC=0
DT_WEATHGEN=1800.
WEATHGEN_PRECIP_EXACT=n
DUMP_WEATHER=n
INTER_LIN=n
#
# lenth of simulation :
#------------------------------------------------------------------------------------
TIME_LENGTH=default
#
# split time step :
#------------------------------------------------------------------------------------
SPLIT_DT=1
TIME_SKIP=0
#
# parameters describing the surface (vegetation + soil) :
#------------------------------------------------------------------------------------
#
SLOWPROC_LAI_TEMPDIAG=280.
#

CONDVEG_SNOWA=default
#
# surface initializtion :
ENERBIL_TSURF=280.
HYDROL_SNOW=0.0
HYDROL_SNOWAGE=0.0
HYDROL_SNOW_NOBIO=0.0
HYDROL_SNOW_NOBIO_AGE=0.0
HYDROL_HDRY=0.0
HYDROL_HUMR=1.0
HYDROL_BQSB=default
HYDROL_GQSB=0.0
HYDROL_DSG=0.0
HYDROL_DSP=default
HYDROL_QSV=0.0
THERMOSOIL_TPRO=280.
DIFFUCO_LEAFCI=233.

# read the LAI :
LAI_MAP=n

HYDROL_CWRR=n
AGRICULTURE=n

RIVER_ROUTING=n
ROUTING_RIVERS=50